DIN Rail Bluetooth 4G Gateway
English Product Documentation
A metal enclosure, external antenna and wide-input DC or PoE power suit industrial Bluetooth data collection. UDP/MQTT transport and OTA maintenance support integration with existing systems.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
The document lists a 4G antenna interface, but the network table specifies LAN. Confirm the 4G backhaul module, configuration and connectivity service when ordering.
IS40B4GDP Series Bluetooth Gateway
Product Specifications
Important Notices
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
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[bookmark: _Toc84583844]1.1 Electrical Specifications
	Power supply
	PoE or DC 12 to 36 V

	Power
	5W

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc84583845]1.2 Technical Specifications
	Main MCU
	32-bit ARM M4

	Operating frequency
	2.4GHz

	Transmit power
	Bluetooth: 10 dBm

	Protocol
	Bluetooth 5.0

	Receiver sensitivity
	BLE:>-104dBm

	Transmission range*
	BLE：300m

	Encryption
	AES encryption supported



Note: Transmission range is specified for line-of-sight conditions.
[bookmark: _Toc84583846]1.3 Physical Specifications
	Dimensions
	Mounting ears folded: 185 x 140 x 30 mm; extended: 210 x 140 x 30 mm. Antenna height: 230 mm.

	Color
	Black

	Weight
	580g

	Material
	Sheet metal

	Ingress protection
	None



[bookmark: _Toc84583847]1.4 Additional Specifications
	Network connection
	10/100 Mbps LAN port

	Network addressing
	DHCP or static IP

	Network transport
	UDP/MQTT

	Antenna
	External fiberglass antenna

	Antenna connector
	N-type female



[bookmark: _Toc84583848]1.5 Configuration Functions
	Destination IP
	Domain name or IP address supported

	Over-the-air update
	OTA supported

	Configuration method
	WeChat mini program or ACServer



	Bluetooth antenna connector
	N-type
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	4G antenna connector
	N-type
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