iBeacon Beacon Series
English Product Documentation
Indoor, industrial-protection and wristband variants support standard iBeacon broadcasts. Configure UUID, Major, Minor, interval and transmit power by phone.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
The source lists up to ten years for indoor/industrial variants and three to six months for the wristband; battery, broadcast configuration and temperature affect endurance. Confirm explosion-protection certificates and scope when selecting a model.
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Product enquiries and technical support: zydc0915@gmail.com
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Important Notices
Copyright
Copyright 2019. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
[bookmark: _Toc208857499][bookmark: _Toc208857498][bookmark: _Toc177638927]JJ-IB32I Indoor Beacon
[bookmark: _Toc177638928]Electrical Specifications
	Battery capacity
	2400mAh

	Peak current
	5.5mA

	Sleep current
	<1uA

	Average current
	<30uA*

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



Average current depends on the broadcast interval and power. The stated default is 500 ms at 0 dBm.
[bookmark: _Toc177638929]Operating frequency
	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc177638930]Physical Specifications
	Dimensions
	53*23mm

	Color
	White

	Weight
	45g

	Housing material
	ABS



Note: Physical specifications vary with the packaging variant.
Colors can be selected for bulk orders; stocked units ship according to availability.
Weight varies slightly by model.
[bookmark: _Toc177638931]Additional Specifications
	Transmit power
	-20 dB to 4 dB in 4 dB steps

	Coverage
	Maximum diameter: 100 m

	Battery life
	Up to 10 years*

	Tamper detection
	Limit-switch tamper detection*

	Water resistance
	IP55

	Security
	AES encryption, tamper protection, connectable and non-connectable modes

	Supported protocols
	Apple standard iBeacon protocol; Bluetooth 5.0



*
Battery life depends on transmit power, transmission interval and ambient temperature.
Optional function; not included in the standard configuration.
[bookmark: _Toc177638932]Configuration Functions
	Phone configuration
	Configure UUID, Major, Minor, broadcast interval, transmit power and tamper-protection key.

	Over-the-air update
	OTA supported
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[bookmark: _Toc177638934]Packaging Specifications
48 units per carton
[bookmark: _Toc177638935]JJ-IB100 Explosion Protected Beacon
[bookmark: _Toc177638936]Electrical Specifications
	Battery capacity
	2600 mAh; optional 5200 mAh. Default: 2600 mAh.

	Peak current
	5.5mA

	Sleep current
	<1uA

	Average current
	<30uA*

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



Average current depends on the broadcast interval and power. The stated default is 500 ms at 0 dBm.
[bookmark: _Toc177638937]Operating frequency
	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc177638938]Physical Specifications
	Dimensions
	120*120*24mm

	Color
	Industrial yellow, black, blue, off-white and other optional colors

	Weight
	185-195g

	Housing material
	Modified ABS



Notes
Colors can be selected for bulk orders; stocked units ship according to availability.
[bookmark: _Toc177638939]Additional Specifications
	Transmit power
	-40dB-4dB

	Coverage
	Maximum diameter: 100 m

	Battery life
	Up to 10 years with maximum battery capacity

	Water resistance
	IP68

	Compression resistance
	10 tonnes

	Certification
	Explosion-protection certification

	Security
	AES encryption, tamper protection, connectable and non-connectable modes

	Supported protocols
	Apple standard iBeacon protocol; Bluetooth 5.0



[bookmark: _Toc177638940]Configuration Functions
	Phone configuration
	Configure UUID, Major, Minor, broadcast interval, transmit power and tamper-protection key.

	Over-the-air update
	OTA supported
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[bookmark: _Toc177638942]Packaging Specifications
60 units per carton
[bookmark: _Toc177638943]JJ-IB32W Wristband iBeacon
[bookmark: _Toc177638944]Electrical Specifications
	Battery capacity
	50mAh

	Power supply
	Rechargeable lithium battery

	Charging method
	Mirco usb

	Charging voltage
	5V

	Peak current
	5.5mA

	Sleep current
	<1uA

	Average current
	<30uA*

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



Average current depends on the broadcast interval and power. The stated default is 500 ms at 0 dBm.
[bookmark: _Toc177638945]Operating frequency
	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc177638946]Physical Specifications
	Dimensions
	250*40*11mm

	Color
	White, pink, blue, black, orange or green

	Weight
	30g

	Housing material
	Plastic



Note: Colors can be selected for bulk orders; stocked units ship according to availability.
[bookmark: _Toc177638947]Additional Specifications
	Transmit power
	-40dB-4dB

	Coverage
	Maximum diameter: 100 m

	Battery life
	3 to 6 months

	Water resistance
	IP53

	Security
	AES encryption, tamper protection, connectable and non-connectable modes

	Supported protocols
	Apple standard iBeacon protocol; Bluetooth 5.0



[bookmark: _Toc177638948]Configuration Functions
	Phone configuration
	Configure UUID, Major, Minor, broadcast interval, transmit power and tamper-protection key.

	Over-the-air update
	OTA supported
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