Clip On Anti Tamper Asset Tag
English Product Documentation
A compact clip-on tag for asset tracking and finding. Supports AoA positioning, remote LED indication, tamper alerts and motion sensing for tools, returnable items and medical equipment.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
Sub-meter positioning requires compatible AoA gateways and a positioning platform. Actual accuracy depends on obstructions and deployment geometry.
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Jinju Intelligence Beijing Technology Co Ltd - Haidian Beijing
Date: 1 October 2021
Product enquiries and technical support: zydc0915@gmail.com
Revision History
	Version
	Changes
	Author
	Reviewer
	Date

	V1.0.0
	Initial release
	
	
	21.10.01



Important Notices
Copyright
Copyright 2021 Jinju Intelligence Beijing Technology Co Ltd. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
[bookmark: _Toc209790642]Chapter 1 JJ-IP32BC Tamper Detecting Asset Tag Specifications
The JJ-IP asset tag series is designed by Jinju Intelligence for asset visibility and lean management. It combines location tracking with AoA positioning, active finding and intelligent status sensing for logistics, manufacturing, healthcare and enterprise IT asset management.
Core Functions and Applications
Submeter AoA Positioning
Function: Bluetooth 5.1 Angle of Arrival positioning supports indoor accuracy of 0.5 to 1 m.
Application: Finer location detail than traditional Bluetooth zone estimates helps users find a particular shelf, tool, laboratory instrument or medical device and reduce search time.
Active Finding with Remote LED Indication
Function: Select an asset ID on the management platform map, or search for the asset and issue a Find command. The corresponding tag responds by flashing its LED.
Application: Identify an asset among dense shelving or equipment. A warehouse operator can trigger the target device to identify itself without checking each item. The source claims an efficiency improvement of more than 90%.
Tamper Alarm
For fixed assets such as high-value instruments, server cabinets and secure storage, removal of the tag triggers an alarm to help protect against unauthorized movement or detachment.
Motion Detection and Configurable Policies
Combined with precise positioning, motion detection records asset tracks and stationary periods for utilization analysis. Adjustable reporting intervals and sensitivity balance tracking requirements and battery life.
Example Applications
Advanced manufacturing: Submeter positioning and active finding for tool carts and precision molds.
Smart warehouses: Precise location management of pallets and boxes, with one-command material finding.
Hospital assets: Locate mobile monitors and infusion pumps; the source describes an audible finding command to help staff retrieve equipment.
Data centers: Cabinet-level server and switch positioning with tamper protection.
[bookmark: _Toc209790643]Electrical Specifications
	Operating voltage
	3.3V

	Battery specification
	1 x CR2450 cell

	Maximum current
	<8.5mA@3.3V

	Listening current
	<3mA@3.3v

	Bluetooth transmit current
	<8.5mA@3.3v

	Sleep current
	<10uA@3.3V

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc209790644]Operating frequency
	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc209790645]Physical Specifications
	Dimensions
	4.3*3.1*3.3cm

	Color
	Yellow

	Weight
	22g

	Housing material
	PC



[bookmark: _Toc209790646]Additional Specifications
	Motion and stationary detection
	Supported

	Low-battery notification
	Flashing LED

	Firmware update
	Individual phone updates or gateway batch updates supported



[bookmark: _Toc209790647]Configuration Functions
	Beacon filtering
	Supported

	Data transmission interval
	Adjustable

	Motion amplitude trigger
	Adjustable sensitivity

	Data transmission after becoming stationary
	Supported



Note: Configuration requires a phone supporting Bluetooth 4.2 or later.
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