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A three-axis sensor adjusts broadcast and positioning frequency according to motion. Pair the tag with a Bluetooth gateway for asset positioning, low-battery monitoring and batch maintenance.
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Important Notices
Copyright
Copyright 2021 Jinju Intelligence Beijing Technology Co Ltd. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
[bookmark: _Toc112690369]Chapter 1 JJ-IP32B Asset Location Tag Specifications
[bookmark: _Toc112690370]1.1 Functions
A built-in three-axis sensor dynamically adjusts broadcast and positioning frequency. Broadcast settings can be configured with a mini program. The high-capacity battery provides more than eight years of maximum stationary standby. An integrated filtering algorithm supports 1 to 3 m positioning with a compatible Bluetooth gateway. Optional buzzer and tamper-detection components enable asset finding and tamper alarms.
[bookmark: _Toc112690371]1.2 Electrical Specifications
	Operating voltage
	3.6V

	Battery specification
	1 x power-type 14505 cell

	Maximum Bluetooth listening current
	<6mA@3.6v

	Maximum Bluetooth transmit current
	<8.5mA@3.6v

	Sleep current
	<10uA@3.6V

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc112690372]1.3 Operating Frequencies
	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc112690373]1.4 Physical Specifications
	Dimensions
	81*41*20mm

	Color
	White

	Weight
	100g

	Housing material
	PC



[bookmark: _Toc112690374]1.5 Additional Specifications
	Motion and stationary detection
	Supported

	Low-battery notification
	Supported

	Firmware update
	Individual updates by phone or batch updates through a gateway



[bookmark: _Toc112690375]1.6 Configuration Functions
	Beacon filtering
	Supported

	Data transmission interval
	Adjustable

	Motion amplitude trigger
	Adjustable sensitivity

	Data transmission after becoming stationary
	Supported



Note: Configuration requires a phone supporting Bluetooth 4.2 or later.
[bookmark: _Toc112690376]1.7 Product Appearance
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