Indoor Bluetooth LoRa Gateway
English Product Documentation
An indoor metal gateway combining Bluetooth and LoRa collection. The SX1301 supports eight uplink channels and one downlink channel for personnel tags and sensor data.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
Classified as indoor according to the filename. One source heading says outdoor, but the protection rating is listed as none; no waterproof capability is claimed. LoRa does not automatically mean LoRaWAN.
JJ-IS40BL Series Bluetooth LoRa Gateway
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Important Notices
Copyright
Copyright 2019 Jinju Intelligence Beijing Technology Co Ltd. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
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[bookmark: _Toc62038832]Electrical Specifications
	Power supply
	POE

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc62038833]Technical Specifications
	Main MCU
	32-bit ARM M4

	Operating frequency
	Bluetooth: 2.4 GHz; LoRa: 480 MHz

	Transmit power
	Bluetooth: 8 dBm; LoRa: 25 dBm

	Protocol
	Bluetooth 5.0; LoRa

	Receiver sensitivity
	BLE:<-101dBm LORA: <-138dBm

	Transmission range*
	BLE：300m ； LORA：1Km

	Device capacity
	BLE: More than 100 nodes scanned per second; LoRa: More than 20 nodes scanned per second

	Encryption
	AES encryption supported

	LoRa channels
	8 uplink channels and 1 downlink channel

	LoRa data rate
	0~37.5kbps

	LoRa controller
	Sx1301



Note: Transmission range is specified for line-of-sight conditions.
[bookmark: _Toc62038834]Physical Specifications
	Dimensions
	Mounting ears folded: 185 x 140 x 30 mm; extended: 210 x 140 x 30 mm. Antenna height: 230 mm.

	Color
	Black

	Weight
	600g

	Material
	Sheet metal

	Ingress protection
	None



[bookmark: _Toc62038835]Additional Specifications
	Network connection
	10/100 Mbps LAN port

	Network addressing
	DHCP or static IP

	Network transport
	UDP

	Antenna
	External magnetic-base antenna

	Antenna connector
	SMA



[bookmark: _Toc62038836]Configuration Functions
	Destination IP
	Domain name or IP address supported

	Over-the-air update
	OTA supported

	Configuration method
	Bluetooth mini program or ACServer



	Bluetooth antenna connector
	SMA connector
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