Indoor AoA Positioning Gateway
English Product Documentation
A Bluetooth 5.1 ceiling gateway for tracking people and assets. Its on-board antenna array measures signal direction, while ACServer handles position calculation, device management and integration with business platforms.
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Selection Notes
Software capabilities also reference the AoA gateway technical manual. Accuracy assumes unobstructed conditions; validate mounting height, target height and obstructions on site.
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Important Notices
Copyright
Copyright 2019 Jinju Intelligence Beijing Technology Co Ltd. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
[bookmark: _Toc78208384]Chapter 1 JJ-IS40BAXP Bluetooth 5.1 AoA Indoor Ceiling Gateway
[bookmark: _Toc78208385]1.1 Electrical Specifications
	Item
	Specification

	Power supply
	PoE or DC 5 V / 1 A

	Rated power
	3W

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc78208386]1.2 Technical Specifications
	Item
	Specification

	Main MCU
	Dual-core ARM M4F at 64 MHz

	Flash
	1MB+512KB

	RAM
	256KB+128B

	Frequency
	2.4Ghz 

	Protocol
	Bluetooth 5.1 and 4.2

	Data rate
	250 Kbps, 1 Mbps and 2 Mbps supported

	Transmit power
	10dBm；

	Receiver sensitivity
	>-95dBm

	Encryption
	Hardware AES encryption supported



[bookmark: _Toc78208387]1.3 Physical Specifications
	Item
	Specification

	Dimensions
	230*230*40mm

	Color
	White

	Weight
	500g

	Housing material
	ABS



[bookmark: _Toc78208388]1.4 Additional Specifications
	Network connection
	10/100 Mbps LAN port

	Network addressing
	DHCP or static IP

	Network transport
	UDP

	Antenna
	On-board antenna array



[bookmark: _Toc78208389]1.5 Configuration Functions
	Destination IP
	Domain name or IP address supported

	Over-the-air update
	OTA supported

	Configuration method
	WeChat mini program or ACServer



[bookmark: _Toc78208390]1.6 Bluetooth Functions
	AoA coverage
	Circular coverage with radius 1.5 times the installation height

	AoA accuracy
	Within 0.5 m in unobstructed conditions

	Bluetooth 5.1 support
	Yes

	Positioning with earlier Bluetooth versions
	Yes

	Bluetooth data transmission support
	Yes



[bookmark: _Toc78208391]1.7 Product Appearance
[image: ]
[bookmark: _Toc78208392]1.8 Packaging Specifications
Samples: One unit per carton with cardboard and EPE foam. Bulk orders: Fifty bagged units per carton.
[bookmark: _Toc78208393]1.9 Product Logo
Neutral packaging by default; custom logos available.
[bookmark: _Toc78208394]1.10 Accessories
Power adapter not included by default; purchase separately.
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