Multi Mode Personnel Badge
English Product Documentation
A personnel badge for indoor and outdoor management. Bluetooth and LoRa are supported; UWB, BeiDou and access or meal-card functions depend on the model. Magnetic charging, voice and vibration simplify daily use.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
UWB, BeiDou and access functions are model options. Verify explosion-protection certificates and environmental suitability for the shipped device. The illustration represents appearance and is not a display-function commitment.
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Personnel Location Badge Product Brochure
Models: IR-T10A / B / C
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Jinju Beijing Technology Co Ltd
1 Product Overview
The Jinju personnel location badge uses low-power Bluetooth, complies with Apple's iBeacon specification and supports other beacon formats. It offers flexible configuration and straightforward operation.
Features
Bluetooth 5.0 and LoRa dual-mode communication provide flexible data transfer.
A built-in 1300 mAh battery supports extended operation.
Built-in short voice messages can be selected for different application scenarios.
Wear around the neck or at the waist.
Phone mini-program configuration simplifies maintenance.
IP67 water protection.
Supports facial-recognition badge dispensers and centralized charging.
Bluetooth, UWB, BeiDou, LoRa and RFID functions can be configured according to requirements.
2 Product Appearance
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3 Applications
Indoor and outdoor personnel and asset positioning
Personnel location management for construction sites, chemical plants and campuses
4 Detailed Technical Specifications
4.1 Electrical Specifications
	Operating voltage
	3.3V~4.2V

	Charging specification
	5V/0.5A

	Transmit power
	BLE：8dBm LORA：17dBm 

	Protocol
	BLE5.0  LORALAN   

	Receiver sensitivity
	BLE:<-101dBm LORA: <-148dBm  

	Maximum current
	<130mA@3.3V

	Listening current
	<6Ma@3.3v

	Sleep current
	<30Ua@3.3V

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing

	Optional positioning and card functions
	iBeacon, AoA, LoRa, meal card and access control
iBeacon, AoA, UWB, BeiDou, LoRa, meal card and access control



[bookmark: _Toc177638937]4.2 Operating Frequencies
	[bookmark: _Toc177638938]LoRa frequency
	470-510MHz

	UWB frequency
	6 to 6.5 GHz, optional

	Bluetooth frequency
	2.4~2.485GHz

	BeiDou frequency
	BDS: 1.5611 GHz, optional

	RFID
	30 to 300 kHz; the chip can also be matched to the project's access-control and meal-card system



4.3 Physical Specifications
	Dimensions
	104x62.5x8.3mm

	Color
	White

	Weight
	80g

	Water resistance
	IP67

	Housing material
	ABS

	Explosion protection
	Supported



[bookmark: _Toc177638939]4.4 Additional Specifications
	Charging method
	Magnetic charging

	Battery
	1000 to 1400 mAh

	Charge protection
	Overcharge protection

	Low-voltage protection
	Battery undervoltage protection

	Emergency alarm
	Supported, with voice and vibration prompts

	Voice announcements
	Multiple built-in short voice messages supported

	Motion and stationary detection
	Supported

	Low-battery notification
	Flashing LED and voice prompt

	Firmware update
	OTA supported



[bookmark: _Toc177638940]4.5 Configuration Functions
	Filtering enable
	Supported

	Transmission frequency
	Supported

	Motion trigger
	High, normal or low sensitivity

	Transmission duration after becoming stationary
	Supported



5 Packaging
60 units per carton
6 Packing List
	Accessory
	IR-T10A/B/C

	
	Safety-mode location tag

	Main tag
	1 piece

	Lanyard
	1 piece

	Magnetic charging cable
	1 piece

	Certificate of conformity
	1 copy



7 Ordering Information
	Product name
	Model
	Main functions
	Notes

	Personnel location badge
	IR-T10A
	iBeacon, AoA, LoRa, meal card and access control
	

	Personnel location badge
	IR-T10B
	iBeacon, AoA, UWB, BeiDou and LoRa
	

	Personnel location badge
	IR-T10C
	iBeacon, AoA, UWB, BeiDou, LoRa, meal card and access control
	

	Personnel location badge
	IR-T10D
	iBeacon, AoA, BeiDou and LoRa
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