Smart Helmet Location Terminal
English Product Documentation
A helmet-worn Bluetooth LoRa terminal with emergency alarms, voice and vibration prompts. Motion sensing and configurable reporting adapt to field work.
Jinju Intelligence (Beijing) Technology Co., Ltd. | zydc0915@gmail.com
Selection Notes
The specification explicitly lists BLE and LoRa. UWB or satellite positioning is not assumed to be standard from the model name.
Product Specifications
Product: Smart Helmet Location Terminal
Model: JJ-IH32UGRL
Jinju Intelligence Beijing Technology Co Ltd - Beijing
Date: 27 December 2023
Product enquiries and technical support: zydc0915@gmail.com
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Important Notices
Copyright
Copyright 2023. All rights reserved.
No Warranty
No express or implied representation or warranty is made concerning this document. No liability is accepted for merchantability, fitness for a particular purpose, or indirect, special or consequential loss.
Confidentiality
This document, including its attachments, contains confidential information. The recipient acknowledges its confidential nature and may use it only for the specified purpose. It must not be disclosed to any third party.
[bookmark: _Toc118386316]Electrical Specifications
	Operating voltage
	3.3V~4.2V

	Charging specification
	5V/0.5A

	Transmit power
	BLE：8dBm LORA：17dBm

	Protocol
	BLE5.0  LORALAN

	Receiver sensitivity
	BLE:<-101dBm LORA: <-148dBm

	Maximum current
	<130mA@3.3V

	Listening current
	<6Ma@3.3v

	Sleep current
	<30Ua@3.3V

	Operating temperature
	-20℃—60℃

	Operating humidity
	0 to 95%, non-condensing



[bookmark: _Toc118386317]Operating frequency
	LoRa frequency
	470-510MHz

	Bluetooth frequency
	2.4~2.485GHz



[bookmark: _Toc118386318]Physical Specifications
	Dimensions
	65*57*30/72*84*32

	Color
	Yellow

	Weight
	70g

	Water resistance
	IP67

	Housing material
	ABS



[bookmark: _Toc118386319]Additional Specifications
	Charging method
	USB Type-C charging

	Charge protection
	Overcharge protection

	Low-voltage protection
	Battery undervoltage protection

	Emergency alarm
	Supported, with voice and vibration prompts

	Motion and stationary detection
	Supported

	Low-battery notification
	Flashing LED and voice prompt

	Firmware update
	OTA supported



[bookmark: _Toc118386320]Configuration Functions
	Filtering enable
	Supported

	Transmission frequency
	Supported

	Motion trigger
	High, normal or low sensitivity

	Transmission duration after becoming stationary
	Supported



Note: Configuration requires a phone supporting Bluetooth 4.2 or later.
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